Sellection criteria for fully contained events

cut number or events ±500μsec, decay-e cut 107892 HE trigger 36560 Σ_{300nsec} p.e. ≥ 200 p.e. 18902 flasher cuts 18617 F.C.(N_{hitac} < 10) 108 goodness of the fit > 0 107 E_{visible} > 30MeV 100 eye-scan 94 −0.2μsec ≤ T_{GP S} ≤ 1.3μsec 91 D_{wall} ≥ 2m 56